<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.3.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="98.278" y2="0" width="0" layer="20"/>
<wire x1="98.278" y1="0" x2="98.278" y2="46.152" width="0" layer="20"/>
<wire x1="98.278" y1="46.152" x2="0" y2="46.152" width="0" layer="20"/>
<wire x1="0" y1="46.152" x2="0" y2="0" width="0" layer="20"/>
<text>Solder Reflow Oven
By: Zachary Goode</text>
<text>+</text>
<text>+</text>
<text>-</text>
<text>-</text>
<text>-</text>
<text>I/O</text>
<text>I/O</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="0207/7">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 7.5 mm</description>
</package>
</packages>
</library>
<library name="SparkFun-Retired">
<description>&lt;h3&gt;SparkFun Electronics' Retired foot prints&lt;/h3&gt;
In this library you'll find all manner of retired footprints for resistors, capacitors, board names, ICs, etc., that are &lt;b&gt; no longer used&lt;/b&gt; in our catalog.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE-PTH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="con-wago-500">
<description>&lt;b&gt;Wago Screw Clamps&lt;/b&gt;&lt;p&gt;
Grid 5.00 mm&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="W237-103">
<description>&lt;b&gt;WAGO SCREW CLAMP&lt;/b&gt;</description>
</package>
<package name="W237-102">
<description>&lt;b&gt;WAGO SCREW CLAMP&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="con-samtec">
<description>&lt;b&gt;Samtec Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TSW-102-XX-G-S">
<description>&lt;b&gt;THROUGH-HOLE .025" SQ POST HEADER&lt;/b&gt;&lt;p&gt;
Source: Samtec TSW.pdf</description>
</package>
</packages>
</library>
<library name="ArduinoNanoV30">
<packages>
<package name="ARDUINO_NANO">
<description>&lt;b&gt;Arduino Nano V3.0 Module&lt;/b&gt;

&lt;p&gt;The Nano was designed and is being produced by &lt;a href="http://www.gravitech.us/arna30wiatp.html"&gt;Gravitech&lt;/a&gt;.&lt;/p&gt;&lt;br&gt;</description>
</package>
</packages>
</library>
<library name="con-molex">
<description>&lt;b&gt;Molex Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="70543-16">
<description>&lt;b&gt;2.54mm Pitch SL™ Header, Single Row, Vertical, 3.05mm Pocket, Shrouded, 17 Circuits, 0.38µm Gold (Au) Selective Plating, Tin (Sn) PC Tail Plating&lt;/b&gt;&lt;p&gt;&lt;a href =http://www.molex.com/pdm_docs/sd/705430016_sd.pdf&gt;Datasheet &lt;/a&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R1" library="adafruit" package="0207/7" value="4.7K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="adafruit" package="0207/7" value="4.7K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="adafruit" package="0207/7" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="adafruit" package="0207/7" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="adafruit" package="0207/7" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="adafruit" package="0207/7" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="adafruit" package="0207/7" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S1" library="SparkFun-Retired" package="TACTILE-PTH" value="">
<attribute name="NAME"/>
</element>
<element name="S2" library="SparkFun-Retired" package="TACTILE-PTH" value="">
<attribute name="NAME"/>
</element>
<element name="S3" library="SparkFun-Retired" package="TACTILE-PTH" value="">
<attribute name="NAME"/>
</element>
<element name="S4" library="SparkFun-Retired" package="TACTILE-PTH" value="">
<attribute name="NAME"/>
</element>
<element name="S5" library="SparkFun-Retired" package="TACTILE-PTH" value="">
<attribute name="NAME"/>
</element>
<element name="ALWAYSONOFF" library="con-wago-500" package="W237-103" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="237-103"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="18M7116"/>
<attribute name="VALUE"/>
</element>
<element name="5V+" library="con-wago-500" package="W237-102" value="5V+">
<attribute name="MF" value=""/>
<attribute name="MPN" value="237-102"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="70K9898"/>
</element>
<element name="SSR" library="con-wago-500" package="W237-102" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="237-102"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="70K9898"/>
<attribute name="VALUE"/>
</element>
<element name="100KTHERMISTOR" library="con-samtec" package="TSW-102-XX-G-S" value="TSW-102-08-G-S">
<attribute name="MF" value="Samtec Inc."/>
<attribute name="MPN" value="TSW-102-07-G-S"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value=""/>
<attribute name="OC_NEWARK" value=""/>
</element>
<element name="ARDUINO_NANO1" library="ArduinoNanoV30" package="ARDUINO_NANO" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LCD" library="con-molex" package="70543-16" value="C-GRID-16-70543">
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="ARDUINO_NANO1" pad="30"/>
<contactref element="LCD" pad="4"/>
</signal>
<signal name="N$2">
<contactref element="ARDUINO_NANO1" pad="29"/>
<contactref element="LCD" pad="6"/>
</signal>
<signal name="N$3">
<contactref element="ARDUINO_NANO1" pad="20"/>
<contactref element="LCD" pad="14"/>
</signal>
<signal name="N$4">
<contactref element="ARDUINO_NANO1" pad="21"/>
<contactref element="LCD" pad="13"/>
</signal>
<signal name="N$5">
<contactref element="ARDUINO_NANO1" pad="22"/>
<contactref element="LCD" pad="12"/>
</signal>
<signal name="N$6">
<contactref element="ARDUINO_NANO1" pad="23"/>
<contactref element="LCD" pad="11"/>
</signal>
<signal name="N$7">
<contactref element="R1" pad="1"/>
<contactref element="LCD" pad="3"/>
</signal>
<signal name="N$9">
<contactref element="S5" pad="2"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="R6" pad="2"/>
<contactref element="S4" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="S3" pad="2"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="R4" pad="2"/>
<contactref element="S2" pad="2"/>
</signal>
<signal name="N$13">
<contactref element="S1" pad="2"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$14">
<contactref element="S1" pad="1"/>
<contactref element="ARDUINO_NANO1" pad="24"/>
</signal>
<signal name="N$15">
<contactref element="S2" pad="1"/>
<contactref element="ARDUINO_NANO1" pad="25"/>
</signal>
<signal name="N$16">
<contactref element="S3" pad="1"/>
<contactref element="ARDUINO_NANO1" pad="26"/>
</signal>
<signal name="N$17">
<contactref element="S4" pad="1"/>
<contactref element="ARDUINO_NANO1" pad="27"/>
</signal>
<signal name="N$18">
<contactref element="S5" pad="1"/>
<contactref element="ARDUINO_NANO1" pad="28"/>
</signal>
<signal name="N$19">
<contactref element="ALWAYSONOFF" pad="2"/>
<contactref element="ARDUINO_NANO1" pad="16"/>
</signal>
<signal name="N$20">
<contactref element="SSR" pad="1"/>
<contactref element="ARDUINO_NANO1" pad="1"/>
</signal>
<signal name="N$21">
<contactref element="R2" pad="2"/>
<contactref element="100KTHERMISTOR" pad="2"/>
<contactref element="ARDUINO_NANO1" pad="4"/>
</signal>
<signal name="GND">
<contactref element="ARDUINO_NANO1" pad="14"/>
</signal>
<signal name="VIN">
<contactref element="ARDUINO_NANO1" pad="15"/>
</signal>
<signal name="N$8">
<contactref element="S5" pad="3"/>
<contactref element="S4" pad="3"/>
<contactref element="S3" pad="3"/>
<contactref element="S2" pad="3"/>
<contactref element="S1" pad="3"/>
<contactref element="S1" pad="4"/>
<contactref element="S2" pad="4"/>
<contactref element="S3" pad="4"/>
<contactref element="S4" pad="4"/>
<contactref element="S5" pad="4"/>
<contactref element="ALWAYSONOFF" pad="3"/>
<contactref element="5V+" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="ARDUINO_NANO1" pad="12"/>
<contactref element="LCD" pad="2"/>
<contactref element="LCD" pad="15"/>
<contactref element="ARDUINO_NANO1" pad="3"/>
</signal>
<signal name="N$22">
<contactref element="ALWAYSONOFF" pad="1"/>
<contactref element="5V+" pad="2"/>
<contactref element="SSR" pad="2"/>
<contactref element="100KTHERMISTOR" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="ARDUINO_NANO1" pad="19"/>
<contactref element="LCD" pad="1"/>
<contactref element="LCD" pad="5"/>
<contactref element="LCD" pad="16"/>
<contactref element="R3" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="R6" pad="1"/>
<contactref element="R7" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
