// CAPACITIVE SENSOR -----> WAVE SHIELD

#include <FatReader.h>
#include <SdReader.h>
#include <avr/pgmspace.h>
#include "WaveUtil.h"
#include "WaveHC.h"

SdReader card;    // This object holds the information for the card
FatVolume vol;    // This holds the information for the partition on the card
FatReader root;   // This holds the information for the filesystem on the card
FatReader f;      // This holds the information for the file we're play
WaveHC wave;      // This is the only wave (audio) object, since we will only play one at a time

//#define tijuana "TIJUANA.WAV"

//*************THINGS DECLARED*************************

//int val = 0; // the sensor is connected to analogue port 0
//int sonar; 
//int sonar = 0;   

 // lines from code: HumanCircuitLED
 int sensorPin = A0;
 int sensorValue = 0;
 
 // line from code:BORDER
 long time; 

//**********************************************************

// this handy function will return the number of bytes currently free in RAM, great for debugging!   
int freeRam(void)
{
  extern int  __bss_end; 
  extern int  *__brkval; 
  int free_memory; 
  if((int)__brkval == 0) {
    free_memory = ((int)&free_memory) - ((int)&__bss_end); 
  }
  else {
    free_memory = ((int)&free_memory) - ((int)__brkval); 
  }
  return free_memory; 
} 

void sdErrorCheck(void)
{
  if (!card.errorCode()) return;
  putstring("\n\rSD I/O error: ");
  Serial.print(card.errorCode(), HEX);
  putstring(", ");
  Serial.println(card.errorData(), HEX);
  while(1);
}

  // set up serial port
  void setup() {
  Serial.begin(9600);           // set up Serial library at 9600 bps
  Serial.println("Wave Shield TEST ");
  
  putstring("Free RAM: ");       // This can help with debugging, running out of RAM is bad
  Serial.println(freeRam());      // if this is under 150 bytes it may spell trouble!
  
  //line of code from: HumanCircuitLED
  pinMode(sensorPin,INPUT);
  
  // Set the output pins for the DAC control. This pins are defined in the library
  pinMode(2, OUTPUT);
  pinMode(3, OUTPUT);
  pinMode(4, OUTPUT);
  pinMode(5, OUTPUT);
 
randomSeed(analogRead(0));
  
  if (!card.init()) {         //play with 8 MHz spi (default faster!)  
    putstring_nl("Card init. failed!");  // Something went wrong, lets print out why
    sdErrorCheck();
    while(1);                            // then 'halt' - do nothing!
  }
  
  // enable optimize read - some cards may timeout. Disable if you're having problems
  card.partialBlockRead(true);
 
// Now we will look for a FAT partition!
  uint8_t part;
  for (part = 0; part < 5; part++) {     // we have up to 5 slots to look in
    if (vol.init(card, part)) 
      break;                             // we found one, lets bail
  }
  if (part == 5) {                       // if we ended up not finding one  :(
    putstring_nl("No valid FAT partition!");
    sdErrorCheck();      // Something went wrong, lets print out why
    while(1);                            // then 'halt' - do nothing!
  }
  
  // Lets tell the user about what we found
  putstring("Using partition ");
  Serial.print(part, DEC);
  putstring(", type is FAT");
  Serial.println(vol.fatType(),DEC);     // FAT16 or FAT32?
  
  // Try to open the root directory
  if (!root.openRoot(vol)) {
    putstring_nl("Can't open root dir!"); // Something went wrong,
    while(1);                             // then 'halt' - do nothing!
  }
  
  // Whew! We got past the tough parts.
  putstring_nl("Ready!");
}
 
//**********************************************************

void loop(){
   // read the value from the sensor:
  sensorValue = analogRead(sensorPin); 
  //Print the value to the Serial monitor   
  Serial.println(sensorValue);  
  if(sensorValue>50){
   playfile("NOPAL.WAV"); 
  }else{
   wave.stop(); 
  }
  
}

//void loop() {
//   
//    distsensor = 0;
//    for (i=0; i<8; i++) {
//    distsensor += analogRead(0);
//    delay(50);
//    }
//    distsensor /= 8;
//    
//    Serial.print(F("Sensor = ")); Serial.println(distsensor);
//    
//    if (distsensor < 70) {
//       //playcomplete("TIJUANA.WAV");
//       playfile("TIJUANA.WAV");       
//       } else {
//       wave.stop();
//       }
//       delay(1000);
//}

// Plays a full file from beginning to end with no pause.
void playcomplete(char *name) {
  // call our helper to find and play this name
  playfile(name);
  while (wave.isplaying) {
  // do nothing while its playing
  }
  // now its done playing
}

void playfile(char *name) {
  // see if the wave object is currently doing something
  if (wave.isplaying) {// already playing something, so stop it!
//    wave.stop(); // stop it
    return;
  }
  // look in the root directory and open the file
  if (!f.open(root, name)) {
    putstring("Couldn't open file "); Serial.print(name); return;
  }
  // OK read the file and turn it into a wave object
  if (!wave.create(f)) {
    putstring_nl("Not a valid WAV"); return;
  }
  
  // ok time to play! start playback
  wave.play();
}