<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.3.0">
<drawing>
<board>
<plain>
<wire x1="5.08" y1="-3.81" x2="96.5" y2="-3.81" width="0" layer="20"/>
<wire x1="96.5" y1="-3.81" x2="96.5" y2="65.71" width="0" layer="20"/>
<wire x1="96.5" y1="65.71" x2="5.08" y2="65.71" width="0" layer="20"/>
<wire x1="5.08" y1="65.71" x2="5.08" y2="-3.81" width="0" layer="20"/>
<hole x="15.24" y="57.15" drill="0.35"/>
<hole x="15.24" y="54.61" drill="0.35"/>
<hole x="15.24" y="52.07" drill="0.35"/>
<hole x="15.24" y="49.53" drill="0.35"/>
<hole x="15.24" y="46.99" drill="0.35"/>
<hole x="55.88" y="58.42" drill="0.35"/>
<hole x="58.42" y="58.42" drill="0.35"/>
<hole x="66.04" y="49.53" drill="0.35"/>
<hole x="66.04" y="46.99" drill="0.35"/>
<hole x="66.04" y="44.45" drill="0.35"/>
<hole x="68.58" y="44.45" drill="0.35"/>
<hole x="68.58" y="46.99" drill="0.35"/>
<hole x="68.58" y="49.53" drill="0.35"/>
<hole x="27.94" y="3.81" drill="0.35"/>
<hole x="30.48" y="3.81" drill="0.35"/>
<hole x="33.02" y="3.81" drill="0.35"/>
<hole x="35.56" y="3.81" drill="0.35"/>
<hole x="38.1" y="3.81" drill="0.35"/>
<hole x="40.64" y="3.81" drill="0.35"/>
<hole x="43.18" y="3.81" drill="0.35"/>
<hole x="45.72" y="3.81" drill="0.35"/>
<hole x="48.26" y="3.81" drill="0.35"/>
<hole x="50.8" y="3.81" drill="0.35"/>
<hole x="53.34" y="3.81" drill="0.35"/>
<hole x="55.88" y="3.81" drill="0.35"/>
<hole x="58.42" y="3.81" drill="0.35"/>
<hole x="60.96" y="3.81" drill="0.35"/>
<hole x="63.5" y="3.81" drill="0.35"/>
<hole x="66.04" y="3.81" drill="0.35"/>
<hole x="41.91" y="62.23" drill="0.35"/>
<hole x="44.45" y="62.23" drill="0.35"/>
</plain>
<libraries>
<library name="atmel">
<description>&lt;b&gt;AVR Devices&lt;/b&gt;&lt;p&gt;
Configurable logic, microcontrollers, nonvolatile memories&lt;p&gt;
Based on the following sources:&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;www.atmel.com
&lt;li&gt;CD-ROM : Configurable Logic Microcontroller Nonvolatile Memory
&lt;li&gt;CadSoft download site, www.cadsoft.de or www.cadsoftusa.com , file at90smcu_v400.zip
&lt;li&gt;avr.lbr
&lt;/ul&gt;
&lt;author&gt;Revised by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
</packages>
</library>
<library name="avr-7">
<description>&lt;b&gt;AVR Devices&lt;/b&gt;&lt;p&gt;
Version 7 - August 1, 2011.&lt;br&gt;&lt;br&gt;
Added ATmega164P/324P/644P devices for DIP and TQFP.
&lt;p&gt;
Version 4 - March 11, 2008.&lt;br&gt;&lt;br&gt;
This library now includes ONLY ATMEL AVR microcontrollers.  It is the result of merging all other available device libraries available at http://www.cadsoft.de/download as of the time it was made.  In addition to the legacy AT90* devices, it includes most ATMEGA devices including the new 48/88/168, most ATTiny devices and a set of ISP and JTAG pin headers.&lt;p&gt;
Based on the following sources:&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;www.atmel.com
&lt;li&gt; file at90smcu_v400.zip
&lt;li&gt;avr.lbr and atmel.lbr as provided by CadSoft
&lt;li&gt;avr-1.lbr by David Blundell
&lt;li&gt;avr-2.lbr by Boris Zalokar
&lt;li&gt;avr-3.lbr by Carson Reynolds
&lt;li&gt;attiny24_44_84.lbr by Pawel Szramowski (ATTiny24/44/84 devices)
&lt;li&gt;atmel.lbr by Bob Starr (ISP headers)
&lt;li&gt;moates_custom_parts.lbr (edge ISP)
&lt;li&gt;other misc sources
&lt;/ul&gt;
&lt;author&gt;Revised by David Blundell (blundar at gmail dot com) and others.&lt;/author&gt;
&lt;p&gt;
&lt;author&gt;Added Mega162, Tiny2313 John Lussmyer (cougar at casadelgato.com)&lt;/author&gt;
&lt;p&gt;
&lt;author&gt;Added XMega A1,A3,A4,D3,D4 John Lussmyer Aug 1, 2011(cougar at casadelgato.com)&lt;/author&gt;</description>
<packages>
<package name="AVR-ISP-6">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;&lt;p&gt; JTAG 6 Pin, 0.1" Straight</description>
</package>
</packages>
</library>
<library name="eagle_fab">
<packages>
<package name="6MM_SWITCH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
<package name="EFOBM">
</package>
<package name="R1206FAB">
</package>
<package name="LED1206FAB">
<description>LED1206 FAB style (smaller pads to allow trace between)</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Capacitors&lt;/h3&gt;
This library contains capacitors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603">
<description>&lt;p&gt;&lt;b&gt;Generic 1608 (0603) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X05">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X16">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X01">
<description>&lt;h3&gt;Plated Through Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:1&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_01&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="atmel" package="TQFP32-08" value="MEGA8-AI">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATMEGA8-16AU"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="9171371"/>
<attribute name="OC_NEWARK" value="73M8863"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="avr-7" package="AVR-ISP-6" value="AVR-ISP-6VERT">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S1" library="eagle_fab" package="6MM_SWITCH" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="eagle_fab" package="EFOBM" value="RESONATOR"/>
<element name="R1" library="eagle_fab" package="R1206FAB" value="10k">
<attribute name="NAME"/>
</element>
<element name="JP2" library="pinhead" package="1X05" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP3" library="pinhead" package="1X16" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="0603" value="100pF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-11015"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="SparkFun-Capacitors" package="0603" value="1uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-11015"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="SparkFun-Capacitors" package="0603" value="10uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-11015"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="eagle_fab" package="R1206FAB" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="eagle_fab" package="R1206FAB" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J4" library="SparkFun-Connectors" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="eagle_fab" package="R1206FAB" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$2" library="eagle_fab" package="LED1206FAB" value="LEDFAB1206">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$8">
<contactref element="IC1" pad="14"/>
</signal>
<signal name="N$19">
<contactref element="IC1" pad="23"/>
</signal>
<signal name="N$20">
<contactref element="IC1" pad="24"/>
</signal>
<signal name="N$21">
<contactref element="IC1" pad="25"/>
</signal>
<signal name="N$22">
<contactref element="IC1" pad="26"/>
</signal>
<signal name="PIN27">
<contactref element="IC1" pad="27"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="JP1" pad="2"/>
<contactref element="IC1" pad="4"/>
<contactref element="IC1" pad="6"/>
<contactref element="R1" pad="1"/>
<contactref element="JP2" pad="2"/>
<contactref element="JP3" pad="4"/>
<contactref element="C6" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="R2" pad="1"/>
<contactref element="IC1" pad="18"/>
</signal>
<signal name="MOSI">
<contactref element="JP1" pad="4"/>
<contactref element="IC1" pad="15"/>
<contactref element="JP3" pad="8"/>
</signal>
<signal name="GND">
<contactref element="JP1" pad="6"/>
<contactref element="IC1" pad="3"/>
<contactref element="IC1" pad="5"/>
<contactref element="IC1" pad="21"/>
<contactref element="U$1" pad="2"/>
<contactref element="S1" pad="3"/>
<contactref element="S1" pad="4"/>
<contactref element="JP2" pad="1"/>
<contactref element="JP3" pad="3"/>
<contactref element="JP3" pad="5"/>
<contactref element="JP3" pad="7"/>
<contactref element="C6" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="R3" pad="2"/>
<contactref element="U$2" pad="1"/>
</signal>
<signal name="RST">
<contactref element="JP1" pad="5"/>
<contactref element="IC1" pad="29"/>
<contactref element="R1" pad="2"/>
<contactref element="S1" pad="1"/>
<contactref element="S1" pad="2"/>
</signal>
<signal name="SCK">
<contactref element="JP1" pad="3"/>
<contactref element="IC1" pad="17"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="MISO">
<contactref element="JP1" pad="1"/>
<contactref element="IC1" pad="16"/>
<contactref element="JP3" pad="6"/>
</signal>
<signal name="XTAL1">
<contactref element="IC1" pad="7"/>
<contactref element="U$1" pad="1"/>
</signal>
<signal name="XTAL2">
<contactref element="IC1" pad="8"/>
<contactref element="U$1" pad="3"/>
</signal>
<signal name="PIN28">
<contactref element="IC1" pad="28"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="PIN8">
<contactref element="IC1" pad="12"/>
<contactref element="JP3" pad="13"/>
</signal>
<signal name="PIN7">
<contactref element="IC1" pad="11"/>
<contactref element="JP3" pad="14"/>
</signal>
<signal name="PIN6">
<contactref element="IC1" pad="10"/>
<contactref element="JP3" pad="15"/>
</signal>
<signal name="PIN5">
<contactref element="IC1" pad="9"/>
<contactref element="JP3" pad="16"/>
</signal>
<signal name="PIN4">
<contactref element="JP2" pad="3"/>
<contactref element="IC1" pad="2"/>
</signal>
<signal name="PIN3">
<contactref element="JP2" pad="4"/>
<contactref element="IC1" pad="1"/>
</signal>
<signal name="PIN2">
<contactref element="JP2" pad="5"/>
<contactref element="IC1" pad="32"/>
</signal>
<signal name="N$38">
<contactref element="IC1" pad="13"/>
</signal>
<signal name="N$1">
<contactref element="JP3" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="JP3" pad="2"/>
</signal>
<signal name="N$24">
<contactref element="JP3" pad="11"/>
</signal>
<signal name="N$25">
<contactref element="JP3" pad="12"/>
</signal>
<signal name="TX">
<contactref element="J3" pad="1"/>
<contactref element="IC1" pad="31"/>
</signal>
<signal name="RX">
<contactref element="J4" pad="1"/>
<contactref element="IC1" pad="30"/>
</signal>
<signal name="N$3">
<contactref element="R4" pad="2"/>
<contactref element="U$2" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
