<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="68.5" y1="1" x2="8.5" y2="1" width="0.254" layer="20"/>
<wire x1="8.5" y1="1" x2="2" y2="7.5" width="0.254" layer="20" curve="105"/>
<wire x1="2" y1="7.5" x2="2" y2="42.5" width="0.254" layer="20"/>
<wire x1="2" y1="42.5" x2="8.5" y2="49" width="0.254" layer="20" curve="105"/>
<wire x1="8.5" y1="49" x2="68.5" y2="49" width="0.254" layer="20"/>
<wire x1="68.5" y1="49" x2="75" y2="42.5" width="0.254" layer="20" curve="105"/>
<wire x1="75" y1="42.5" x2="75" y2="7.5" width="0.254" layer="20"/>
<wire x1="75" y1="7.5" x2="68.5" y2="1" width="0.254" layer="20" curve="105"/>
<text></text>
<text>Tx</text>
<text>Rx</text>
<text>3v3</text>
<text>Gnd</text>
<text>3v3</text>
<text>Gnd</text>
<hole x="63.5" y="45" drill="3.2"/>
<text>10K</text>
<text>Reset</text>
<text>ATMega328</text>
<text>Beth's Dad 2015</text>
<text>WTV-020</text>
<hole x="63.5" y="5" drill="3.2"/>
<hole x="13.5" y="5" drill="3.2"/>
<hole x="13.5" y="45" drill="3.2"/>
<hole x="15.438" y="38" drill="3.2"/>
<hole x="19.068" y="38" drill="3.2"/>
<text>Switch</text>
<text>Batt</text>
<text>+  -</text>
<text>Charger</text>
<text>+  -</text>
<text>Prog</text>
<text>Player 2</text>
<text>Player 1</text>
<text>Spkr</text>
<text>MCP1825s</text>
<text>"Pongsole"</text>
<text>100nf</text>
<text>100nf</text>
<text>22pf</text>
<text>22pf</text>
<text>8MHz</text>
<text>220uf</text>
<text>220uf</text>
<text>Spkr</text>
<text>100R</text>
<text>100R</text>
<text>+ -</text>
<text>ADC</text>
<text>SD Card</text>
<text>"Pongsole"</text>
<text>"Pongsole"</text>
<text>Beth's Dad
2015 v1.1</text>
<text>See Instructables user
"Ugifer" for firmware etc.</text>
<text>Ugi 2015</text>
</plain>
<libraries>
<library name="rcl">
<packages>
<package name="C025-025X050">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 2.5 x 5 mm</description>
</package>
<package name="0207/10">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 10 mm</description>
</package>
<package name="E2,5-6">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.54 mm, diameter 6 mm</description>
</package>
</packages>
</library>
<library name="crystal">
<packages>
<package name="HC49/S">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="atmel">
<packages>
<package name="DIL28-3">
<description>&lt;B&gt;Dual In Line&lt;/B&gt; 0.3 inch</description>
</package>
</packages>
</library>
<library name="switch-omron">
<description>&lt;b&gt;Omron Switches&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="B3F-10XX">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="1X06-CLEAN">
</package>
</packages>
</library>
<library name="solpad">
<description>&lt;b&gt;Solder Pads/Test Points&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="LSP10">
<description>&lt;b&gt;SOLDER PAD&lt;/b&gt;&lt;p&gt;
drill 1.0 mm</description>
</package>
</packages>
</library>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02">
</package>
</packages>
</library>
<library name="pot">
<description>&lt;b&gt;Potentiometers&lt;/b&gt;&lt;p&gt;
Beckman, Copal, Piher, Spectrol, Schukat&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="3RP/1610N">
<description>&lt;b&gt;16mm Potentiometer&lt;/b&gt; one level&lt;p&gt;
Source: http://www.alphapotentiometers.net/html/16mm_pot_2.html</description>
</package>
</packages>
</library>
<library name="UgiLib 2012-11-03">
<packages>
<package name="1X08SMALL">
<description>Tight Pin Header Package</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X02">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="linear">
<description>&lt;b&gt;Linear Devices&lt;/b&gt;&lt;p&gt;
Operational amplifiers,  comparators, voltage regulators, ADCs, DACs, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO220V">
<description>&lt;b&gt;TO 200 vertical&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
</packages>
</library>
<library name="con-garry">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;a href="www.mpe-connector.de"&gt;Menufacturer&lt;/a&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="332-02">
<description>&lt;b&gt;2 Pin - 2mm Dual Row&lt;/b&gt;&lt;p&gt;
Source: www.mpe-connector.de / garry_shortform_2012.pdf</description>
</package>
</packages>
</library>
<library name="con-molex">
<description>&lt;b&gt;Molex Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="53047-02">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;&lt;p&gt;
wire to board 1.25 mm (.049 inch) pitch header&lt;p&gt;
straight&lt;br&gt;
Sourcxe: http://www.molex.com/pdm_docs/sd/530470210_sd.pdf</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R1" library="rcl" package="0207/10" value="">
<attribute name="VALUE"/>
</element>
<element name="C5" library="rcl" package="C025-025X050" value="">
<attribute name="VALUE"/>
</element>
<element name="C6" library="rcl" package="C025-025X050" value="">
<attribute name="VALUE"/>
</element>
<element name="XTAL1" library="crystal" package="HC49/S" value="">
<attribute name="VALUE"/>
</element>
<element name="PROG" library="adafruit" package="1X06-CLEAN" value="">
<attribute name="VALUE"/>
</element>
<element name="IC1" library="atmel" package="DIL28-3" value="MEGA8-P">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="NAME"/>
</element>
<element name="C3" library="rcl" package="C025-025X050" value="">
<attribute name="VALUE"/>
</element>
<element name="S1" library="switch-omron" package="B3F-10XX" value="">
<attribute name="OC_NEWARK" value="36M3542"/>
<attribute name="MPN" value="B3F-1000"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="176432"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="rcl" package="E2,5-6" value="">
<attribute name="VALUE"/>
</element>
<element name="C4" library="rcl" package="C025-025X050" value="">
<attribute name="VALUE"/>
</element>
<element name="ADC" library="solpad" package="LSP10" value="LSP10">
<attribute name="VALUE"/>
</element>
<element name="JP7" library="SparkFun" package="1X02" value="">
<attribute name="VALUE"/>
</element>
<element name="R2" library="pot" package="3RP/1610N" value=""/>
<element name="R3" library="pot" package="3RP/1610N" value=""/>
<element name="S2" library="switch-omron" package="B3F-10XX" value="">
<attribute name="OC_NEWARK" value="36M3542"/>
<attribute name="MPN" value="B3F-1000"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="176432"/>
<attribute name="VALUE"/>
</element>
<element name="S3" library="switch-omron" package="B3F-10XX" value="">
<attribute name="OC_NEWARK" value="36M3542"/>
<attribute name="MPN" value="B3F-1000"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="176432"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="UgiLib 2012-11-03" package="1X08SMALL" value=""/>
<element name="JP2" library="UgiLib 2012-11-03" package="1X08SMALL" value=""/>
<element name="JP3" library="UgiLib 2012-11-03" package="1X08SMALL" value=""/>
<element name="JP4" library="UgiLib 2012-11-03" package="1X08SMALL" value=""/>
<element name="JP5" library="pinhead" package="1X02" value="">
<attribute name="VALUE"/>
</element>
<element name="IC2" library="linear" package="TO220V" value="786TV"/>
<element name="C1" library="rcl" package="E2,5-6" value="">
<attribute name="VALUE"/>
</element>
<element name="R4" library="rcl" package="0207/10" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP6" library="SparkFun" package="1X02" value="">
<attribute name="VALUE"/>
</element>
<element name="JP8" library="SparkFun" package="1X02" value="">
<attribute name="VALUE"/>
</element>
<element name="R5" library="rcl" package="0207/10" value="">
<attribute name="VALUE"/>
</element>
<element name="LED1" library="led" package="LED3MM" value="">
<attribute name="VALUE"/>
</element>
<element name="X1" library="con-garry" package="332-02" value="332-02"/>
<element name="D12" library="solpad" package="LSP10" value="LSP10">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="A4" library="solpad" package="LSP10" value="LSP10">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="A5" library="solpad" package="LSP10" value="LSP10">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X2" library="con-molex" package="53047-02" value="53047-02">
<attribute name="OC_NEWARK" value="57H4701"/>
<attribute name="MPN" value="53047-0210"/>
<attribute name="MF" value="MOLEX"/>
<attribute name="OC_FARNELL" value="9733051"/>
</element>
<element name="R6" library="rcl" package="0207/10" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="rcl" package="0207/10" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="+3V3">
<contactref element="R1" pad="2"/>
<contactref element="PROG" pad="4"/>
<contactref element="IC1" pad="20"/>
<contactref element="C3" pad="2"/>
<contactref element="PROG" pad="2"/>
<contactref element="IC1" pad="7"/>
<contactref element="C2" pad="+"/>
<contactref element="C4" pad="2"/>
<contactref element="R3" pad="1"/>
<contactref element="JP2" pad="P6"/>
<contactref element="JP1" pad="P6"/>
<contactref element="JP4" pad="P8"/>
<contactref element="IC2" pad="3"/>
<contactref element="R5" pad="1"/>
<contactref element="R2" pad="3"/>
</signal>
<signal name="GND">
<contactref element="C5" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="PROG" pad="3"/>
<contactref element="IC1" pad="22"/>
<contactref element="IC1" pad="8"/>
<contactref element="C3" pad="1"/>
<contactref element="S1" pad="1"/>
<contactref element="C2" pad="-"/>
<contactref element="C4" pad="1"/>
<contactref element="PROG" pad="1"/>
<contactref element="JP7" pad="1"/>
<contactref element="R3" pad="3"/>
<contactref element="S3" pad="4"/>
<contactref element="S3" pad="3"/>
<contactref element="S2" pad="3"/>
<contactref element="S2" pad="4"/>
<contactref element="JP2" pad="P8"/>
<contactref element="JP1" pad="P8"/>
<contactref element="JP3" pad="P8"/>
<contactref element="IC2" pad="2"/>
<contactref element="C1" pad="-"/>
<contactref element="JP6" pad="1"/>
<contactref element="LED1" pad="K"/>
<contactref element="X1" pad="2"/>
<contactref element="X2" pad="2"/>
<contactref element="R2" pad="1"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="RESET">
<contactref element="R1" pad="1"/>
<contactref element="IC1" pad="1"/>
<contactref element="S1" pad="3"/>
</signal>
<signal name="XTAL1">
<contactref element="C6" pad="2"/>
<contactref element="XTAL1" pad="2"/>
<contactref element="IC1" pad="9"/>
</signal>
<signal name="XTAL2">
<contactref element="C5" pad="2"/>
<contactref element="XTAL1" pad="1"/>
<contactref element="IC1" pad="10"/>
</signal>
<signal name="D0">
<contactref element="PROG" pad="5"/>
<contactref element="IC1" pad="2"/>
</signal>
<signal name="D1">
<contactref element="PROG" pad="6"/>
<contactref element="IC1" pad="3"/>
</signal>
<signal name="D4">
<contactref element="IC1" pad="6"/>
<contactref element="JP4" pad="P2"/>
</signal>
<signal name="D13">
<contactref element="IC1" pad="19"/>
<contactref element="JP2" pad="P5"/>
<contactref element="JP1" pad="P5"/>
</signal>
<signal name="AREF">
<contactref element="IC1" pad="21"/>
<contactref element="ADC" pad="MP"/>
</signal>
<signal name="VBATT">
<contactref element="C1" pad="+"/>
<contactref element="IC2" pad="1"/>
<contactref element="JP8" pad="2"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="A0">
<contactref element="IC1" pad="23"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="A1">
<contactref element="IC1" pad="24"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="D6">
<contactref element="S2" pad="2"/>
<contactref element="S2" pad="1"/>
<contactref element="IC1" pad="12"/>
</signal>
<signal name="D7">
<contactref element="S3" pad="2"/>
<contactref element="S3" pad="1"/>
<contactref element="IC1" pad="13"/>
</signal>
<signal name="D12">
<contactref element="IC1" pad="18"/>
<contactref element="D12" pad="MP"/>
</signal>
<signal name="D11">
<contactref element="IC1" pad="17"/>
<contactref element="JP2" pad="P4"/>
<contactref element="JP1" pad="P4"/>
</signal>
<signal name="D10">
<contactref element="IC1" pad="16"/>
<contactref element="JP1" pad="P2"/>
<contactref element="JP2" pad="P2"/>
</signal>
<signal name="D9">
<contactref element="IC1" pad="15"/>
<contactref element="JP1" pad="P1"/>
<contactref element="JP2" pad="P1"/>
</signal>
<signal name="D8">
<contactref element="IC1" pad="14"/>
<contactref element="JP1" pad="P3"/>
<contactref element="JP2" pad="P3"/>
</signal>
<signal name="D2">
<contactref element="JP3" pad="P1"/>
<contactref element="IC1" pad="4"/>
</signal>
<signal name="D3">
<contactref element="JP3" pad="P7"/>
<contactref element="IC1" pad="5"/>
</signal>
<signal name="N$7">
<contactref element="JP5" pad="2"/>
<contactref element="JP3" pad="P5"/>
</signal>
<signal name="A2">
<contactref element="JP4" pad="P7"/>
<contactref element="IC1" pad="25"/>
</signal>
<signal name="D5">
<contactref element="IC1" pad="11"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="BKLT">
<contactref element="R4" pad="2"/>
<contactref element="JP1" pad="P7"/>
<contactref element="JP2" pad="P7"/>
</signal>
<signal name="N$11">
<contactref element="JP7" pad="2"/>
<contactref element="JP8" pad="1"/>
<contactref element="JP6" pad="2"/>
<contactref element="X1" pad="1"/>
<contactref element="X2" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="R5" pad="2"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="N$14">
<contactref element="IC1" pad="27"/>
<contactref element="A4" pad="MP"/>
</signal>
<signal name="N$15">
<contactref element="IC1" pad="28"/>
<contactref element="A5" pad="MP"/>
</signal>
<signal name="N$1">
<contactref element="JP5" pad="1"/>
<contactref element="JP3" pad="P4"/>
</signal>
<signal name="A3">
<contactref element="R6" pad="1"/>
<contactref element="R7" pad="2"/>
<contactref element="IC1" pad="26"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
