Arduino

Reference Language | Libraries | Comparison | Changes

Esplora

## readTemperature()

#### Description

Reads the ambient temperature of the temperature sensor and returns a reading in either the Celsius or Fahrenheit scale, depending on the parameter passed.

#### Syntax

readTemperature(scale)

#### Parameters

scale: the scale of the output, valid arguments are: DEGREES_C and DEGREES_F

#### Returns

int : The temperature reading in Celsius or Fahrenheit. The Celsius range is from -40°C to 150°C, the Fahrenheit range is from -40°F to 302°F.

#### Example

#include <Esplora.h>
void setup()
{
Serial.begin(9600);
}
void loop()
{
int celsius = Esplora.readTemperature(DEGREES_C);
int fahrenheit = Esplora.readTemperature(DEGREES_F);
Serial.print(celsius);
Serial.print("\t");
Serial.print(fahrenheit);
delay(1000);
}
[Get Code]
Reference Home

Corrections, suggestions, and new documentation should be posted to the Forum.

The text of the Arduino reference is licensed under a Creative Commons Attribution-ShareAlike 3.0 License. Code samples in the reference are released into the public domain.

### Share

### This link has expired.
Please re-subscribe to our Newsletters.

### Subscribe to our Newsletters

Email

Please enter a valid email to subscribe

Arduino Newsletter
Arduino Store Newsletter

### Confirm your email address

We need to confirm your email address.
To complete the subscription, please click the link in the email we just sent you.

Thank you for subscribing!

Arduino
via Egeo 16
Torino, 10131
Italy

###### Newsletter

- ©2015 Arduino
- Copyright Notice
- Contact us
- About us
- Careers