Arduino

Reference Language | Libraries | Comparison | Changes

Ethernet : EthernetServer

## EthernetServer()

#### Description

Create a server that listens for incoming connections on the specified port.

#### Syntax

Server(port);

#### Parameters

port: the port to listen on (int)

#### Returns

None

#### Example

#include <SPI.h>
#include <Ethernet.h>
// network configuration. gateway and subnet are optional.
// the media access control (ethernet hardware) address for the shield:
byte mac[] = { 0xDE, 0xAD, 0xBE, 0xEF, 0xFE, 0xED };
//the IP address for the shield:
byte ip[] = { 10, 0, 0, 177 };
// the router's gateway address:
byte gateway[] = { 10, 0, 0, 1 };
// the subnet:
byte subnet[] = { 255, 255, 0, 0 };
// telnet defaults to port 23
EthernetServer server = EthernetServer(23);
void setup()
{
// initialize the ethernet device
Ethernet.begin(mac, ip, gateway, subnet);
// start listening for clients
server.begin();
}
void loop()
{
// if an incoming client connects, there will be bytes available to read:
EthernetClient client = server.available();
if (client == true) {
// read bytes from the incoming client and write them back
// to any clients connected to the server:
server.write(client.read());
}
}
[Get Code]
Reference Home

Corrections, suggestions, and new documentation should be posted to the Forum.

The text of the Arduino reference is licensed under a Creative Commons Attribution-ShareAlike 3.0 License. Code samples in the reference are released into the public domain.

### Share

### This link has expired.
Please re-subscribe to our Newsletters.

### Subscribe to our Newsletters

Email

Please enter a valid email to subscribe

Arduino Newsletter
Arduino Store Newsletter

### Confirm your email address

We need to confirm your email address.
To complete the subscription, please click the link in the email we just sent you.

Thank you for subscribing!

Arduino
via Egeo 16
Torino, 10131
Italy

###### Newsletter

- ©2015 Arduino
- Copyright Notice
- Contact us
- About us
- Careers