Arduino

Reference Language | Libraries | Comparison | Changes

## digitalWrite()

#### Description

Write a HIGH or a LOW value to a digital pin.

If the pin has been configured as an OUTPUT with pinMode(), its voltage will be set to the corresponding value: 5V (or 3.3V on 3.3V boards) for HIGH, 0V (ground) for LOW.

If the pin is configured as an INPUT, digitalWrite() will enable (HIGH) or disable (LOW) the internal pullup on the input pin. It is recommended to set the pinMode() to INPUT_PULLUP to enable the internal pull-up resistor. See the digital pins tutorial for more information.

NOTE: If you do not set the pinMode() to OUTPUT, and connect an LED to a pin, when calling digitalWrite(HIGH), the LED may appear dim. Without explicitly setting pinMode(), digitalWrite() will have enabled the internal pull-up resistor, which acts like a large current-limiting resistor.

#### Syntax

digitalWrite(pin, value)

#### Parameters

pin: the pin number

value: HIGH or LOW

#### Returns

none

#### Example

    int ledPin = 13;                 // LED connected to digital pin 13

    void setup()
    {
      pinMode(ledPin, OUTPUT);      // sets the digital pin as output
    }

    void loop()
    {
      digitalWrite(ledPin, HIGH);   // sets the LED on
      delay(1000);                  // waits for a second
      digitalWrite(ledPin, LOW);    // sets the LED off
      delay(1000);                  // waits for a second
    }

Sets pin 13 to HIGH, makes a one-second-long delay, and sets the pin back to LOW.

#### Note

The analog input pins can be used as digital pins, referred to as A0, A1, etc.

#### See also

- pinMode()
- digitalRead()
- Tutorial: Digital Pins

Reference Home

Corrections, suggestions, and new documentation should be posted to the Forum.

The text of the Arduino reference is licensed under a Creative Commons Attribution-ShareAlike 3.0 License. Code samples in the reference are released into the public domain.

### Share

### This link has expired.
Please re-subscribe to our Newsletters.

### Subscribe to our Newsletters

Email

Please enter a valid email to subscribe

Arduino Newsletter
Arduino Store Newsletter

### Confirm your email address

We need to confirm your email address.
To complete the subscription, please click the link in the email we just sent you.

Thank you for subscribing!

Arduino
via Egeo 16
Torino, 10131
Italy

###### Newsletter

- ©2015 Arduino
- Copyright Notice
- Contact us
- About us
- Careers