(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 76)
    (no_connects 0)
    (area 98.959999 40.539999 199.490001 142.465001)
    (thickness 1.6)
    (drawings 27)
    (tracks 322)
    (zones 0)
    (modules 30)
    (nets 34)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.3)
    (trace_clearance 0.2)
    (zone_clearance 0.4)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 BUZZER)
  (net 2 GND)
  (net 3 +12V)
  (net 4 VREG)
  (net 5 VCC)
  (net 6 "Net-(C4-Pad1)")
  (net 7 "Net-(CONTRAST1-Pad2)")
  (net 8 LCDRS)
  (net 9 LCDE)
  (net 10 LCDD4)
  (net 11 LCDD5)
  (net 12 LCDD6)
  (net 13 LCDD7)
  (net 14 BEC)
  (net 15 "Net-(J1-Pad2)")
  (net 16 TX)
  (net 17 RX)
  (net 18 CURSENS)
  (net 19 "Net-(J4-Pad2)")
  (net 20 "Net-(J6-Pad1)")
  (net 21 "Net-(J6-Pad2)")
  (net 22 "Net-(J6-Pad3)")
  (net 23 ESCSIG)
  (net 24 SDA)
  (net 25 SCL)
  (net 26 "Net-(L1-Pad2)")
  (net 27 MOSI)
  (net 28 RESET)
  (net 29 SCK)
  (net 30 MISO)
  (net 31 TSWITCH)
  (net 32 "Net-(R3-Pad2)")
  (net 33 "Net-(THROTTLE1-Pad2)")
  (net_class Default "To jest domyślna klasa połączeń."
    (clearance 0.2)
    (trace_width 0.3)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net BEC)
    (add_net BUZZER)
    (add_net CURSENS)
    (add_net ESCSIG)
    (add_net GND)
    (add_net LCDD4)
    (add_net LCDD5)
    (add_net LCDD6)
    (add_net LCDD7)
    (add_net LCDE)
    (add_net LCDRS)
    (add_net MISO)
    (add_net MOSI)
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(CONTRAST1-Pad2)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(L1-Pad2)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(THROTTLE1-Pad2)")
    (add_net RESET)
    (add_net RX)
    (add_net SCK)
    (add_net SCL)
    (add_net SDA)
    (add_net TSWITCH)
    (add_net TX)
    (add_net VCC)
    (add_net VREG)
  )
  (net_class "HIGH CURRENT" ""
    (clearance 0.2)
    (trace_width 1)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net "Net-(J6-Pad1)")
    (add_net "Net-(J6-Pad2)")
    (add_net "Net-(J6-Pad3)")
  )
  (module Buzzers_Beepers:Buzzer_12x9.5RM7.6 (layer F.Cu) (tedit 58B1A329)
    (at 135.89 113.03 180)
    (descr "Generic Buzzer, D12mm height 9.5mm with RM7.6mm")
    (tags buzzer)
    (fp_text reference BZ1 (at 3.8 -7.2 180) (layer F.SilkS))
    (fp_text value Buzzer (at 3.8 7.4 180) (layer F.Fab))
    (fp_text user + (at -0.01 -2.54 180) (layer F.Fab))
    (fp_text user + (at -0.01 -2.54 180) (layer F.SilkS))
    (fp_text user %R (at 3.8 -4 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 BUZZER))
    (pad 2 thru_hole circle (at 7.6 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Buzzers_Beepers.3dshapes/Buzzer_12x9.5RM7.6.wrl
      (at (xyz 0.15 0 0))
      (scale (xyz 4 4 4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D3.8mm_W2.6mm_P2.50mm (layer B.Cu) (tedit 597BC7C2)
    (at 186.69 48.26 270)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.8*2.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.8mm width 2.6mm Capacitor")
    (fp_text reference C1 (at 1.25 2.61 270) (layer B.SilkS))
    (fp_text value 330nF (at 1.25 -2.61 270) (layer B.Fab))
    (fp_text user %R (at 1.25 0 270) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 +12V))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.8mm_W2.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D3.8mm_W2.6mm_P2.50mm (layer B.Cu) (tedit 597BC7C2)
    (at 186.69 57.15 90)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.8*2.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.8mm width 2.6mm Capacitor")
    (fp_text reference C2 (at 1.25 2.61 90) (layer B.SilkS))
    (fp_text value 100nF (at 1.25 -2.61 90) (layer B.Fab))
    (fp_text user %R (at 1.25 0 90) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 VREG))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.8mm_W2.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D3.8mm_W2.6mm_P2.50mm (layer B.Cu) (tedit 5ABA379C)
    (at 148.59 83.82 270)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.8*2.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.8mm width 2.6mm Capacitor")
    (fp_text reference C3 (at 3.81 2.54 270) (layer B.SilkS))
    (fp_text value 100nF (at 1.25 -2.61 270) (layer B.Fab))
    (fp_text user %R (at 1.25 0 270) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 VCC))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.8mm_W2.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D3.8mm_W2.6mm_P2.50mm (layer B.Cu) (tedit 5ABA3794)
    (at 120.65 87.63 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.8*2.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.8mm width 2.6mm Capacitor")
    (fp_text reference C4 (at -2.54 0 180) (layer B.SilkS))
    (fp_text value 100nF (at 1.25 -2.61 180) (layer B.Fab))
    (fp_text user %R (at 1.25 0 180) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C4-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.8mm_W2.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometers:Potentiometer_Triwood_RM-065 (layer F.Cu) (tedit 5ABA3769)
    (at 109.22 58.42 270)
    (descr "Potentiometer, Trimmer, RM-065")
    (tags "Potentiometer Trimmer RM-065")
    (fp_text reference CONTRAST1 (at 1.27 -11.43 360) (layer F.SilkS))
    (fp_text value POT (at 7.5 -2.5 360) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 -5.04 270) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 7 "Net-(CONTRAST1-Pad2)"))
    (pad 3 thru_hole circle (at 5 0 270) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 5 VCC))
    (model Potentiometers.3dshapes/Potentiometer_Triwood_RM-065.wrl
      (at (xyz 0 0 0))
      (scale (xyz 4 4 4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 5ABA3751)
    (at 176.53 59.69 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value "POWER SOURCE" (at -2.54 2.54 180) (layer F.Fab))
    (fp_text user %R (at 0 2.54 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 BEC))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 VREG))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 5ABA3776)
    (at 149.86 106.68 270)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33 270) (layer F.SilkS))
    (fp_text value SERIAL (at 2.54 3.81 360) (layer F.Fab))
    (fp_text user %R (at 0 3.81 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 VCC))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 TX))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 RX))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 5ABA377B)
    (at 123.19 107.95 270)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33 270) (layer F.SilkS))
    (fp_text value ACS712 (at 2.54 2.54 360) (layer F.Fab))
    (fp_text user %R (at 0 2.54 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 CURSENS))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 VCC))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Terminal_Blocks:TerminalBlock_Altech_AK300-2_P5.00mm locked (layer F.Cu) (tedit 59FF0306)
    (at 140.97 49.53)
    (descr "Altech AK300 terminal block, pitch 5.0mm, 45 degree angled, see http://www.mouser.com/ds/2/16/PCBMETRC-24178.pdf")
    (tags "Altech AK300 terminal block pitch 5.0mm")
    (fp_text reference J5 (at -1.92 -6.99) (layer F.SilkS))
    (fp_text value "ESC POWER" (at 2.78 7.75) (layer F.Fab))
    (fp_text user %R (at 2.5 -2) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.98 3.96) (drill 1.32) (layers *.Cu *.Mask)
      (net 19 "Net-(J4-Pad2)"))
    (pad 2 thru_hole oval (at 5 0) (size 1.98 3.96) (drill 1.32) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Terminal_Blocks.3dshapes/TerminalBlock_Altech_AK300-2_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Terminal_Blocks:TerminalBlock_Altech_AK300-3_P5.00mm locked (layer F.Cu) (tedit 5ABA376F)
    (at 107.95 49.53)
    (descr "Altech AK300 terminal block, pitch 5.0mm, 45 degree angled, see http://www.mouser.com/ds/2/16/PCBMETRC-24178.pdf")
    (tags "Altech AK300 terminal block pitch 5.0mm")
    (fp_text reference J6 (at 5 -7.1) (layer F.SilkS))
    (fp_text value Motor (at 11.43 7.62) (layer F.Fab))
    (fp_text user %R (at 5 -2) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.98 3.96) (drill 1.32) (layers *.Cu *.Mask)
      (net 20 "Net-(J6-Pad1)"))
    (pad 2 thru_hole oval (at 5 0) (size 1.98 3.96) (drill 1.32) (layers *.Cu *.Mask)
      (net 21 "Net-(J6-Pad2)"))
    (pad 3 thru_hole oval (at 10 0) (size 1.98 3.96) (drill 1.32) (layers *.Cu *.Mask)
      (net 22 "Net-(J6-Pad3)"))
    (model ${KISYS3DMOD}/Terminal_Blocks.3dshapes/TerminalBlock_Altech_AK300-3_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 5ABA3759)
    (at 152.4 45.72 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J7 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value "ESC SIGNAL" (at -2.54 2.54 180) (layer F.Fab))
    (fp_text user %R (at 0 2.54 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 BEC))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 ESCSIG))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Terminal_Blocks:TerminalBlock_Altech_AK300-3_P5.00mm locked (layer F.Cu) (tedit 59FF0306)
    (at 124.46 49.53)
    (descr "Altech AK300 terminal block, pitch 5.0mm, 45 degree angled, see http://www.mouser.com/ds/2/16/PCBMETRC-24178.pdf")
    (tags "Altech AK300 terminal block pitch 5.0mm")
    (fp_text reference J8 (at 5 -7.1) (layer F.SilkS))
    (fp_text value "ESC OUTPUT" (at 4.95 7.3) (layer F.Fab))
    (fp_text user %R (at 5 -2) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.98 3.96) (drill 1.32) (layers *.Cu *.Mask)
      (net 22 "Net-(J6-Pad3)"))
    (pad 2 thru_hole oval (at 5 0) (size 1.98 3.96) (drill 1.32) (layers *.Cu *.Mask)
      (net 21 "Net-(J6-Pad2)"))
    (pad 3 thru_hole oval (at 10 0) (size 1.98 3.96) (drill 1.32) (layers *.Cu *.Mask)
      (net 20 "Net-(J6-Pad1)"))
    (model ${KISYS3DMOD}/Terminal_Blocks.3dshapes/TerminalBlock_Altech_AK300-3_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 5ABA377F)
    (at 114.3 107.95 270)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J9 (at 0 -2.33 270) (layer F.SilkS))
    (fp_text value HX711 (at 2.54 3.81 360) (layer F.Fab))
    (fp_text user %R (at 0 3.81 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 SDA))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 SCL))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 VCC))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5ABA375D)
    (at 166.37 45.72 270)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (fp_text reference J10 (at 0 -2.33 270) (layer F.SilkS))
    (fp_text value XT60 (at 2.54 1.27 360) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +12V))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Inductors_THT:L_Axial_L5.3mm_D2.2mm_P7.62mm_Horizontal_Vishay_IM-1 (layer B.Cu) (tedit 5ABA378F)
    (at 113.03 83.82)
    (descr "L, Axial series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.3*2.2mm^2, Vishay, IM-1, http://www.vishay.com/docs/34030/im.pdf")
    (tags "L Axial series Axial Horizontal pin pitch 7.62mm  length 5.3mm diameter 2.2mm Vishay IM-1")
    (fp_text reference L1 (at 1.27 2.54) (layer B.SilkS))
    (fp_text value 10uH (at 3.81 -2.16) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 VCC))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(L1-Pad2)"))
    (model Inductors_THT.3dshapes/L_Axial_L5.3mm_D2.2mm_P7.62mm_Horizontal_Vishay_IM-1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Multicomp:Multicomp_MC9A12-1034_2x05x2.54mm_Straight (layer F.Cu) (tedit 5ABA374A)
    (at 156.21 60.96)
    (descr http://www.farnell.com/datasheets/1520732.pdf)
    (tags "connector multicomp MC9A MC9A12")
    (fp_text reference PROGRAMMER1 (at 5.08 -6.35) (layer F.SilkS))
    (fp_text value AVR-ISP-10 (at 5.08 5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 MOSI))
    (pad 2 thru_hole circle (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 VCC))
    (pad 3 thru_hole circle (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at 2.54 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at 5.08 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 RESET))
    (pad 6 thru_hole circle (at 5.08 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 7 thru_hole circle (at 7.62 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 SCK))
    (pad 8 thru_hole circle (at 7.62 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 9 thru_hole circle (at 10.16 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 MISO))
    (pad 10 thru_hole circle (at 10.16 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 137.16 99.06 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R1 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value 10K (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 VCC))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 28 RESET))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 176.53 109.22 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R2 (at 0 -1.85 270) (layer F.SilkS))
    (fp_text value 10K (at 0 1.9 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 31 TSWITCH))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 154.94 81.28)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R3 (at 0 -1.85) (layer F.SilkS))
    (fp_text value R (at 0 1.9) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 +12V))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(R3-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 154.94 83.82 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R4 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value R (at 0 1.9 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(R3-Pad2)"))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_NV_B03P-NV_3x5.00mm_Vertical (layer F.Cu) (tedit 59DBB535)
    (at 182.88 119.38 90)
    (descr "JST NV series connector, B03P-NV, 5.00mm pitch, top entry type, through hole")
    (tags "connector jst nv vertical")
    (fp_text reference SW1 (at 5 -4.8 90) (layer F.SilkS))
    (fp_text value SWITCH (at 5 6 90) (layer F.Fab))
    (fp_text user %R (at 5 2.5 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.35 3) (drill 1.65) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 5 0 90) (size 2.35 3) (drill 1.65) (layers *.Cu *.Mask)
      (net 5 VCC))
    (pad 3 thru_hole oval (at 10 0 90) (size 2.35 3) (drill 1.65) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad2)"))
    (model ${KISYS3DMOD}/Connectors_JST.3dshapes/JST_NV_B03P-NV_3x5.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_THT:SW_PUSH_6mm locked (layer F.Cu) (tedit 5923F252)
    (at 165.1 106.68)
    (descr https://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (tags "tact sw push 6mm")
    (fp_text reference SW2 (at 3.25 -2) (layer F.SilkS))
    (fp_text value BUTTON (at 3.75 6.7) (layer F.Fab))
    (fp_text user %R (at 3.25 2.25) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 31 TSWITCH))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 VCC))
    (pad 2 thru_hole circle (at 6.5 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 31 TSWITCH))
    (pad 1 thru_hole circle (at 6.5 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 VCC))
    (model ${KISYS3DMOD}/Buttons_Switches_THT.3dshapes/SW_PUSH_6mm.wrl
      (at (xyz 0.005 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometers:Potentiometer_Alps_RK163_Single_Vertical (layer F.Cu) (tedit 58826D68)
    (at 158.75 123.19 270)
    (descr "Potentiometer, vertically mounted, Omeg PC16PU, Omeg PC16PU, Omeg PC16PU, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GH/249GH Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148A/149A Single with mounting plates, Vishay/Spectrol 148/149 Double, Vishay/Spectrol 148A/149A Double with mounting plates, Piher PC-16 Single, Piher PC-16 Single, Piher PC-16 Single, Piher PC-16SV Single, Piher PC-16 Double, Piher PC-16 Triple, Piher T16H Single, Piher T16L Single, Piher T16H Double, Alps RK163 Single, http://www.alps.com/prod/info/E/PDF/Potentiometer/MetalShaft/RK163/RK163.PDF")
    (tags "Potentiometer vertical  Omeg PC16PU  Omeg PC16PU  Omeg PC16PU  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GH/249GH Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148A/149A Single with mounting plates  Vishay/Spectrol 148/149 Double  Vishay/Spectrol 148A/149A Double with mounting plates  Piher PC-16 Single  Piher PC-16 Single  Piher PC-16 Single  Piher PC-16SV Single  Piher PC-16 Double  Piher PC-16 Triple  Piher T16H Single  Piher T16L Single  Piher T16H Double  Alps RK163 Single")
    (fp_text reference THROTTLE1 (at 0 -15.2 270) (layer F.SilkS))
    (fp_text value POT (at 0 5.2 270) (layer F.Fab))
    (pad 3 thru_hole circle (at 0 -10 270) (size 2.34 2.34) (drill 1.3) (layers *.Cu *.Mask)
      (net 5 VCC))
    (pad 2 thru_hole circle (at 0 -5 270) (size 2.34 2.34) (drill 1.3) (layers *.Cu *.Mask)
      (net 33 "Net-(THROTTLE1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.34 2.34) (drill 1.3) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Potentiometers.3dshapes/Potentiometer_Alps_RK163_Single_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-220-3_Vertical (layer F.Cu) (tedit 58CE52AD)
    (at 181.61 48.26 270)
    (descr "TO-220-3, Vertical, RM 2.54mm")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference U1 (at 2.54 -3.62 270) (layer F.SilkS))
    (fp_text value L7805 (at 2.54 3.92 270) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.62 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 3 +12V))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 4 VREG))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_QFP:TQFP-32_7x7mm_Pitch0.8mm (layer F.Cu) (tedit 58CC9A48)
    (at 135.89 87.63 180)
    (descr "32-Lead Plastic Thin Quad Flatpack (PT) - 7x7x1.0 mm Body, 2.00 mm [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (attr smd)
    (fp_text reference U2 (at 0 -6.05 180) (layer F.SilkS))
    (fp_text value ATMEGA8-16AU (at 0 6.05 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -4.25 -2.8 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 9 LCDE))
    (pad 2 smd rect (at -4.25 -2 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 8 LCDRS))
    (pad 3 smd rect (at -4.25 -1.2 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -4.25 -0.4 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 5 VCC))
    (pad 5 smd rect (at -4.25 0.4 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at -4.25 1.2 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 5 VCC))
    (pad 7 smd rect (at -4.25 2 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at -4.25 2.8 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at -2.8 4.25 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 10 LCDD4))
    (pad 10 smd rect (at -2 4.25 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 11 LCDD5))
    (pad 11 smd rect (at -1.2 4.25 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 12 LCDD6))
    (pad 12 smd rect (at -0.4 4.25 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 13 LCDD7))
    (pad 13 smd rect (at 0.4 4.25 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 23 ESCSIG))
    (pad 14 smd rect (at 1.2 4.25 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 31 TSWITCH))
    (pad 15 smd rect (at 2 4.25 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 27 MOSI))
    (pad 16 smd rect (at 2.8 4.25 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 30 MISO))
    (pad 17 smd rect (at 4.25 2.8 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 29 SCK))
    (pad 18 smd rect (at 4.25 2 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(L1-Pad2)"))
    (pad 19 smd rect (at 4.25 1.2 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 20 smd rect (at 4.25 0.4 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C4-Pad1)"))
    (pad 21 smd rect (at 4.25 -0.4 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 22 smd rect (at 4.25 -1.2 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 23 smd rect (at 4.25 -2 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(THROTTLE1-Pad2)"))
    (pad 24 smd rect (at 4.25 -2.8 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(R3-Pad2)"))
    (pad 25 smd rect (at 2.8 -4.25 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 18 CURSENS))
    (pad 26 smd rect (at 2 -4.25 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 27 smd rect (at 1.2 -4.25 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 24 SDA))
    (pad 28 smd rect (at 0.4 -4.25 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 25 SCL))
    (pad 29 smd rect (at -0.4 -4.25 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 28 RESET))
    (pad 30 smd rect (at -1.2 -4.25 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 17 RX))
    (pad 31 smd rect (at -2 -4.25 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 16 TX))
    (pad 32 smd rect (at -2.8 -4.25 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 BUZZER))
    (model ${KISYS3DMOD}/Housings_QFP.3dshapes/TQFP-32_7x7mm_Pitch0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Displays:WC1602A (layer F.Cu) (tedit 5958D986)
    (at 115.57 69.85)
    (descr "LCD 16x2 http://www.wincomlcd.com/pdf/WC1602A-SFYLYHTC06.pdf")
    (tags "LCD 16x2 Alphanumeric 16pin")
    (fp_text reference U3 (at -5.82 -3.81) (layer F.SilkS))
    (fp_text value RC1602A (at -4.31 34.66) (layer F.Fab))
    (fp_text user %R (at 30.37 14.74) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 5 VCC))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 7 "Net-(CONTRAST1-Pad2)"))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 8 LCDRS))
    (pad 5 thru_hole oval (at 10.16 0) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole oval (at 12.7 0) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 9 LCDE))
    (pad 7 thru_hole oval (at 15.24 0) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 17.78 0) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask))
    (pad 9 thru_hole oval (at 20.32 0) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask))
    (pad 10 thru_hole oval (at 22.86 0) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask))
    (pad 11 thru_hole oval (at 25.4 0) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 10 LCDD4))
    (pad 12 thru_hole oval (at 27.94 0) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 11 LCDD5))
    (pad 13 thru_hole oval (at 30.48 0) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 12 LCDD6))
    (pad 14 thru_hole oval (at 33.02 0) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 13 LCDD7))
    (pad 15 thru_hole oval (at 35.56 0) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 5 VCC))
    (pad 16 thru_hole oval (at 38.1 0) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad "" thru_hole circle (at -5.4991 0) (size 3 3) (drill 2.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -5.4991 31.0007) (size 3 3) (drill 2.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 69.49948 31.0007) (size 3 3) (drill 2.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 69.5 0) (size 3 3) (drill 2.5) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Displays.3dshapes/WC1602A.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x01_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 144.78 62.23 180)
    (descr "Through hole straight pin header, 2x01, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x01 2.54mm double row")
    (fp_text reference J4 (at 1.27 -2.33 180) (layer F.SilkS))
    (fp_text value "CURRENT SENSOR" (at 1.27 2.33 180) (layer F.Fab))
    (fp_text user %R (at 1.27 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +12V))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J4-Pad2)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Symbols:KiCad-Logo2_8mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 175.26 92.71 180)
    (descr "KiCad Logo")
    (tags "Logo KiCad")
    (attr virtual)
    (fp_text reference REF*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value KiCad-Logo2_8mm_SilkScreen (at 0.75 0 180) (layer B.Fab) hide)
  )
  (module Symbols:OSHW-Logo2_14.6x12mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 144.78 120.65 180)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference REF*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value OSHW-Logo2_14.6x12mm_SilkScreen (at 0.75 0 180) (layer B.Fab) hide)
  )
  (gr_circle (center 128.27 63.5) (end 129.54 63.5) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 173.99 64.77) (end 173.99 66.04) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 176.53 123.19) (end 177.8 123.19) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 106.68 123.19) (end 107.95 123.19) (layer Edge.Cuts) (width 0.15))
  (gr_text " DESIGNED IN CORK" (at 123.19 121.92) (layer B.SilkS))
  (gr_text NIKODEMBARTNIK.PL (at 172.72 85.09) (layer B.SilkS))
  (gr_text "THRUST STAND V1" (at 173.99 81.28) (layer B.SilkS))
  (gr_text "NIKODEM BARTNIK\n27.03.2018" (at 173.99 76.2) (layer B.SilkS))
  (gr_line (start 193.04 124.46) (end 193.04 121.92) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 186.69 124.46) (end 193.04 124.46) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 193.04 46.99) (end 193.04 121.92) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 186.69 46.99) (end 186.69 40.64) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 105.41 130.81) (end 186.69 130.81) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 105.41 40.64) (end 186.69 40.64) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 99.06 124.46) (end 99.06 46.99) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 105.41 124.46) (end 105.41 130.81) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 105.41 46.99) (end 99.06 46.99) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.4) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 100.33 124.46) (xy 100.33 46.99) (xy 105.41 41.91) (xy 186.69 41.91) (xy 191.77 46.99)
        (xy 191.77 124.46) (xy 186.69 129.54) (xy 105.41 129.54)
      )
    )
  )
  (zone (net 5) (net_name VCC) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.4))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.4) (thermal_bridge_width 0.4))
    (polygon
      (pts
        (xy 191.77 46.99) (xy 191.77 124.46) (xy 186.69 129.54) (xy 105.41 129.54) (xy 100.33 124.46)
        (xy 100.33 46.99) (xy 105.41 41.91) (xy 186.69 41.91)
      )
    )
  )
)
