Display
- (x1) CEM3491BY (0.39" Common Anode 4-Digit 7-Segment Display Amber Color)
- (x1) MAX7219 (Led driver display)
- (x1) 10k Resistor
- (x1) 10uF Capacitor
- (x1) XH2.54-5P (5Pin Straight PCB Male Box Header Bar Connector)

Controller
- (x1) STM8S005C6T6 (Microcontroller)
- (x1) ESP8266-12 (WiFi module)
- (x1) ASM1117-5.0 (voltage regulators 5V)
- (x1) ASM1117-3.3 (voltage regulators 3V3)
- (x1) 470uF Capacitor
- (x1) 1uF Capacitor
- (x3) 10uF Capacitor
- (x2) 4.7k Resistor
- (x1) Mini Pushbutton Switch (4Pin)
- (x1) SW-420 (Vibration sensor)
- (x1) DS1307 (Real Time Clock)
- (x1) 32.768 khz crystal
- (x1) CR2032 battery
- (x1) CR2032 battery holder
- (x2) XH2.54-2P (2Pin Straight PCB Male Box Header Bar Connector)
- (x1) XH2.54-5P (5Pin Straight PCB Male Box Header Bar Connector)
- (x1) XH2.54-4P (4Pin Straight PCB Male Box Header Bar Connector)
- (x2) Cable Double Connector XH2.54-2P
- (x1) Cable Double Connector XH2.54-5P
- (x1) Cable Double Connector XH2.54-4P

External interactive
- (x1) PCB prototype double side
- (x1) DHT22 (Temperature, Humidity sensor)
- (x1) C1815 Transistor
- (x1) XH2.54-4P (4Pin Straight PCB Male Box Header Bar Connector)
- (x1) DC power jack
- (x1) Buzzer 5V
- (x1) Rocker Switch On/Off

Other
- (x9) M2 bolt
- (x1) 9V adapter
- (x1) ST-LINK
- heat sink tube
- wood veneer