Bounce2

bounce2buttons.ino

Example of two instances of the Bounce class that switches the debug LED when either one of the two buttons is pressed.

/*
DESCRIPTION
====================
Simple example of the Bounce library that switches the debug LED when
either of 2 buttons are pressed.
*/
// Include the Bounce2 library found here :
// https://github.com/thomasfredericks/Bounce2
#include <Bounce2.h>
#define BUTTON_PIN_1 2
#define BUTTON_PIN_2 3
#define LED_PIN 13
// Instantiate a Bounce object
Bounce debouncer1 = Bounce();
// Instantiate another Bounce object
Bounce debouncer2 = Bounce();
void setup() {
// Setup the first button with an internal pull-up :
pinMode(BUTTON_PIN_1,INPUT_PULLUP);
// After setting up the button, setup the Bounce instance :
debouncer1.attach(BUTTON_PIN_1);
debouncer1.interval(5); // interval in ms
// Setup the second button with an internal pull-up :
pinMode(BUTTON_PIN_2,INPUT_PULLUP);
// After setting up the button, setup the Bounce instance :
debouncer2.attach(BUTTON_PIN_2);
debouncer2.interval(5); // interval in ms
//Setup the LED :
pinMode(LED_PIN,OUTPUT);
}
void loop() {
// Update the Bounce instances :
debouncer1.update();
debouncer2.update();
// Get the updated value :
int value1 = debouncer1.read();
int value2 = debouncer2.read();
// Turn on the LED if either button is pressed :
if ( value1 == LOW || value2 == LOW ) {
digitalWrite(LED_PIN, HIGH );
}
else {
digitalWrite(LED_PIN, LOW );
}
}