Updating the Flip USB Driver - Windows XP

Flip uses a new USB driver since the release 3.1.0

These detailed instructions will show you how to update the Flip USB driver from the Jungo driver to the libUsb one.

1 - Open the Device Manager and right-click the Atmel USB device in the Jungo section.

In the pop-up menu, select Update Driver.

2 - In the Hardware Update Wizard dialog, select the "No, not this time" option. Click Next >

3 - Select the Install from a list or specific location option. Click Next >

4 - Select the Don't search. I will choose the driver to install option. Click Next >

5 - Click the Have Disk button.

6 - Click the Browse button to navigate to the Flip \usb folder; it contains the INF file. Click the OK button.

7 - Click Finish.

8 - The Device Manager updates and shows the Atmel device in the LibUSB-Win32 Devices section.